TABLE 4-7.5. OPTIONAL MUSIC/MULTIMEDIA ROOM

|  |  |
| --- | --- |
| **Description/ Usage** | This optional room is smaller than the basic activity room module and is used for musical instrument instruction for one to two students or as a video and/or photography lab. |
| **Min. Ceiling Ht.** | 2.44 m (8 ft.). |
| **Finishes** | **Walls.**  Painted CMU or other material with consideration for acoustical separation from adjacent spaces.  Navy and Air Force do not permit CMU in these spaces. |
|  | **Floor.** VCT or Carpet with vinyl or rubber base. |
|  | **Ceiling.** ACP. |
| **Plumbing** | None required. |
| **HVAC** | 20 C (68 F) minimum, 26 C (78 F) maximum. |
| **Fire Protection** | Provide system per paragraph 3-5.3. |
| **Power** | Provide outlets per code. |
| **Lighting** | 540 Lux (50 ft. candles). |
| **Communication** | **CCTV.** Provide at least one outlet.  **CATV/Internal Video.** None required.  **PA/Audio.** Provide a speaker.  **Telephone.** None required.  Army requires one line with two-way internal communication.  **Data.**  None required.  **Security.** Provide a vision panel in the door. |
| **Casework** | None required. |
| **Furnishings Fixtures & Equipment (FF&E)** | May include chairs, music stands, etc. |
| **Special Requirements** | Integrate equipment storage spaces with the design of these rooms.  Music rooms require acoustical separation from the remainder of the facility. Provide soundproof walls from floor to roof deck. Consider providing an acoustical vestibule at the entrance to this room or, at a minimum, a door with sound gaskets on all edges.  Provide a vision panel in the door. |
| For use during project execution by the appropriate Service agency | |
| **Occupancy** | Staff. |
|  | Patrons/Youth. |
| **Min. net m2 (ft2)** |  |